RDM630 is better than RDM6300\_but the price is 10 times higher

Tx output of RDM6300 is 3.3v tolerance: high is 3.2-3.3

Low is 0

So you don’t need a voltage shifter to transfer signal into esp32!